interface Vlan10

ip access-group RESTRICT\_INTER\_VLAN in

!

interface Vlan20

ip access-group RESTRICT\_INTER\_VLAN in

!

interface Vlan30

ip access-group RESTRICT\_INTER\_VLAN in

!

interface Vlan40

ip access-group RESTRICT\_INTER\_VLAN in

!

interface Vlan50

ip access-group RESTRICT\_INTER\_VLAN in

!

interface Vlan60

ip access-group RESTRICT\_INTER\_VLAN in

!

interface Vlan70

ip access-group RESTRICT\_INTER\_VLAN in

ip access-list extended RESTRICT\_INTER\_VLAN

! Autoriser tout le trafic depuis VLAN10 (administratif) pour les réseaux 172.32 et 172.33

permit ip 172.32.10.0 0.0.0.255 any

permit ip 172.33.10.0 0.0.0.255 any

! Autoriser tout le trafic vers et depuis le serveur vidéo

permit ip any host 172.33.30.50

permit ip host 172.33.30.50 any

! (Autres règles RTMP ou spécifiques peuvent être supprimées si la règle ci-dessus répond au besoin)

! --- Règles de blocage inter-VLAN pour le réseau 172.32 ---

deny ip 172.32.20.0 0.0.0.255 172.32.20.0 0.0.0.255

deny ip 172.32.20.0 0.0.0.255 172.32.30.0 0.0.0.255

deny ip 172.32.20.0 0.0.0.255 172.32.40.0 0.0.0.255

deny ip 172.32.20.0 0.0.0.255 172.32.50.0 0.0.0.255

deny ip 172.32.20.0 0.0.0.255 172.32.60.0 0.0.0.255

deny ip 172.32.20.0 0.0.0.255 172.32.70.0 0.0.0.255

deny ip 172.32.30.0 0.0.0.255 172.32.20.0 0.0.0.255

deny ip 172.32.30.0 0.0.0.255 172.32.30.0 0.0.0.255

deny ip 172.32.30.0 0.0.0.255 172.32.40.0 0.0.0.255

deny ip 172.32.30.0 0.0.0.255 172.32.50.0 0.0.0.255

deny ip 172.32.30.0 0.0.0.255 172.32.60.0 0.0.0.255

deny ip 172.32.30.0 0.0.0.255 172.32.70.0 0.0.0.255

deny ip 172.32.40.0 0.0.0.255 172.32.20.0 0.0.0.255

deny ip 172.32.40.0 0.0.0.255 172.32.30.0 0.0.0.255

deny ip 172.32.40.0 0.0.0.255 172.32.40.0 0.0.0.255

deny ip 172.32.40.0 0.0.0.255 172.32.50.0 0.0.0.255

deny ip 172.32.40.0 0.0.0.255 172.32.60.0 0.0.0.255

deny ip 172.32.40.0 0.0.0.255 172.32.70.0 0.0.0.255

deny ip 172.32.50.0 0.0.0.255 172.32.20.0 0.0.0.255

deny ip 172.32.50.0 0.0.0.255 172.32.30.0 0.0.0.255

deny ip 172.32.50.0 0.0.0.255 172.32.40.0 0.0.0.255

deny ip 172.32.50.0 0.0.0.255 172.32.50.0 0.0.0.255

deny ip 172.32.50.0 0.0.0.255 172.32.60.0 0.0.0.255

deny ip 172.32.50.0 0.0.0.255 172.32.70.0 0.0.0.255

deny ip 172.32.60.0 0.0.0.255 172.32.20.0 0.0.0.255

deny ip 172.32.60.0 0.0.0.255 172.32.30.0 0.0.0.255

deny ip 172.32.60.0 0.0.0.255 172.32.40.0 0.0.0.255

deny ip 172.32.60.0 0.0.0.255 172.32.50.0 0.0.0.255

deny ip 172.32.60.0 0.0.0.255 172.32.60.0 0.0.0.255

deny ip 172.32.60.0 0.0.0.255 172.32.70.0 0.0.0.255

deny ip 172.32.70.0 0.0.0.255 172.32.20.0 0.0.0.255

deny ip 172.32.70.0 0.0.0.255 172.32.30.0 0.0.0.255

deny ip 172.32.70.0 0.0.0.255 172.32.40.0 0.0.0.255

deny ip 172.32.70.0 0.0.0.255 172.32.50.0 0.0.0.255

deny ip 172.32.70.0 0.0.0.255 172.32.60.0 0.0.0.255

deny ip 172.32.70.0 0.0.0.255 172.32.70.0 0.0.0.255

! --- Règles de blocage inter-VLAN pour le réseau 172.33 ---

deny ip 172.33.20.0 0.0.0.255 172.33.20.0 0.0.0.255

deny ip 172.33.20.0 0.0.0.255 172.33.30.0 0.0.0.255

deny ip 172.33.20.0 0.0.0.255 172.33.40.0 0.0.0.255

deny ip 172.33.20.0 0.0.0.255 172.33.50.0 0.0.0.255

deny ip 172.33.20.0 0.0.0.255 172.33.60.0 0.0.0.255

deny ip 172.33.20.0 0.0.0.255 172.33.70.0 0.0.0.255

deny ip 172.33.30.0 0.0.0.255 172.33.20.0 0.0.0.255

deny ip 172.33.30.0 0.0.0.255 172.33.30.0 0.0.0.255

deny ip 172.33.30.0 0.0.0.255 172.33.40.0 0.0.0.255

deny ip 172.33.30.0 0.0.0.255 172.33.50.0 0.0.0.255

deny ip 172.33.30.0 0.0.0.255 172.33.60.0 0.0.0.255

deny ip 172.33.30.0 0.0.0.255 172.33.70.0 0.0.0.255

deny ip 172.33.40.0 0.0.0.255 172.33.20.0 0.0.0.255

deny ip 172.33.40.0 0.0.0.255 172.33.30.0 0.0.0.255

deny ip 172.33.40.0 0.0.0.255 172.33.40.0 0.0.0.255

deny ip 172.33.40.0 0.0.0.255 172.33.50.0 0.0.0.255

deny ip 172.33.40.0 0.0.0.255 172.33.60.0 0.0.0.255

deny ip 172.33.40.0 0.0.0.255 172.33.70.0 0.0.0.255

deny ip 172.33.50.0 0.0.0.255 172.33.20.0 0.0.0.255

deny ip 172.33.50.0 0.0.0.255 172.33.30.0 0.0.0.255

deny ip 172.33.50.0 0.0.0.255 172.33.40.0 0.0.0.255

deny ip 172.33.50.0 0.0.0.255 172.33.50.0 0.0.0.255

deny ip 172.33.50.0 0.0.0.255 172.33.60.0 0.0.0.255

deny ip 172.33.50.0 0.0.0.255 172.33.70.0 0.0.0.255

deny ip 172.33.60.0 0.0.0.255 172.33.20.0 0.0.0.255

deny ip 172.33.60.0 0.0.0.255 172.33.30.0 0.0.0.255

deny ip 172.33.60.0 0.0.0.255 172.33.40.0 0.0.0.255

deny ip 172.33.60.0 0.0.0.255 172.33.50.0 0.0.0.255

deny ip 172.33.60.0 0.0.0.255 172.33.60.0 0.0.0.255

deny ip 172.33.60.0 0.0.0.255 172.33.70.0 0.0.0.255

deny ip 172.33.70.0 0.0.0.255 172.33.20.0 0.0.0.255

deny ip 172.33.70.0 0.0.0.255 172.33.30.0 0.0.0.255

deny ip 172.33.70.0 0.0.0.255 172.33.40.0 0.0.0.255

deny ip 172.33.70.0 0.0.0.255 172.33.50.0 0.0.0.255

deny ip 172.33.70.0 0.0.0.255 172.33.60.0 0.0.0.255

deny ip 172.33.70.0 0.0.0.255 172.33.70.0 0.0.0.255

! Autoriser le reste du trafic

permit ip any any

**interface Vlan10**

**no ip helper-address 172.32.10.10**

**interface Vlan20**

**no ip helper-address 172.32.10.10**

**interface Vlan30**

**no ip helper-address 172.32.10.10**

**interface Vlan40**

**no ip helper-address 172.32.10.10**

**interface Vlan50**

**no ip helper-address 172.32.10.10**

**interface Vlan60**

**no ip helper-address 172.32.10.10**

**interface Vlan70**

**no ip helper-address 172.32.10.10**

**ip dhcp excluded-address 172.32.10.1 172.32.10.99**

**ip dhcp excluded-address 172.32.10.201 172.32.10.253**

**! ip dhcp pool VLAN10**

**network 172.32.10.0 255.255.255.0**

**default-router 172.32.10.254**

**dns-server 8.8.8.8 8.8.4.4**

**exit**